**Diving spares and repairs box contents**

* rings (+ tiny watchmakers screwdriver for removal)
* DIN inserts (if you have an A clamp first stage)
* Small adjustable spanner (ideally 2)
* Set of Allen keys (8mm for removing cylinder inserts and 5mm + 4mm for removing/inserting blanks on first stage ports)
* Small tube of silicon grease (for O rings)
* Blanking plugs for first stage ports
* Spare regulator mouthpiece (+ very thin, long cable tie to secure it)
* Large and small cable ties (+ a tool to cut them)
* 1 metre of thin bungee cord
* Strong plastic + metal (brass/stainless steel) clips of various sizes
* Block of beeswax (for dry suit zip)
* Glue for membrane dry suit (e.g. Aquasure) + patches
* Neoprene glue (e.g. Black witch)
* Thin (3mm) and thicker (5mm) braided nylon cord
* “Leatherman” multiple tool
* Lanyards with stainless steel spring toggles

**Possible extras**

* Spare fin strap
* Spare mask strap
* Dive computer manual
* Pocket or wrist slate
* Spare pencil, pencil sharpener + eraser for slate
* Spare computer battery
* Anti-fog spray for mask
* Torch charger/battery
* Velcro strap to tighten loose or splitting neck seal